<session jtag_chain="USB-Blaster [USB-0]" jtag_device="@1: EP3C(10|5)/EP4CE(10|6) (0x020F10DD)" sof_file="">
  <display_tree gui_logging_enabled="0">
    <display_branch instance="auto_signaltap_0" log="USE_GLOBAL_TEMP" signal_set="USE_GLOBAL_TEMP" trigger="USE_GLOBAL_TEMP"/>
  </display_tree>
  <mnemonics/>
  <static_plugin_mnemonics/>
  <instance entity_name="sld_signaltap" is_auto_node="yes" is_expanded="true" name="auto_signaltap_0" source_file="sld_signaltap.vhd">
    <node_ip_info instance_id="0" mfg_id="110" node_id="0" version="6"/>
    <position_info>
      <single attribute="active tab" value="1"/>
      <single attribute="data horizontal scroll position" value="7"/>
      <single attribute="data vertical scroll position" value="0"/>
      <single attribute="zoom level denominator" value="1"/>
      <single attribute="zoom level numerator" value="8"/>
      <single attribute="zoom offset denominator" value="1"/>
      <single attribute="zoom offset numerator" value="16368"/>
    </position_info>
    <signal_set global_temp="1" name="signal_set: 2026/06/01 22:10:31  #0">
      <clock name="CLK50" polarity="posedge" tap_mode="probeonly"/>
      <config is_hps_trigger_out_selected="false" ram_type="AUTO" reserved_data_nodes="0" reserved_storage_qualifier_nodes="0" reserved_trigger_nodes="0" sample_depth="131072" trigger_in_enable="yes" trigger_in_node="clk50_div2" trigger_in_tap_mode="probeonly" trigger_out_enable="no"/>
      <top_entity/>
      <signal_vec>
        <trigger_input_vec>
          <wire name="clk50_div2" tap_mode="probeonly"/>
        </trigger_input_vec>
        <data_input_vec>
          <wire name="clk50_div2" tap_mode="probeonly"/>
        </data_input_vec>
        <storage_qualifier_input_vec>
          <wire name="clk50_div2" tap_mode="probeonly"/>
        </storage_qualifier_input_vec>
      </signal_vec>
      <presentation>
        <unified_setup_data_view>
          <node data_index="0" duplicate_name_allowed="false" is_data_input="true" is_node_valid="true" is_storage_input="true" is_trigger_input="true" level-0="dont_care" name="clk50_div2" pwr_level-0="dont_care" pwr_storage-0="dont_care" pwr_storage-1="dont_care" pwr_storage-2="dont_care" storage-0="dont_care" storage-1="dont_care" storage-2="dont_care" storage_index="0" tap_mode="probeonly" trigger_index="0" type="unknown"/>
        </unified_setup_data_view>
        <data_view>
          <net data_index="0" duplicate_name_allowed="false" is_data_input="true" is_node_valid="true" is_storage_input="true" is_trigger_input="true" level-0="dont_care" name="clk50_div2" pwr_level-0="dont_care" pwr_storage-0="dont_care" pwr_storage-1="dont_care" pwr_storage-2="dont_care" storage-0="dont_care" storage-1="dont_care" storage-2="dont_care" storage_index="0" tap_mode="probeonly" trigger_index="0" type="unknown"/>
        </data_view>
        <setup_view>
          <net data_index="0" duplicate_name_allowed="false" is_data_input="true" is_node_valid="true" is_storage_input="true" is_trigger_input="true" level-0="dont_care" name="clk50_div2" pwr_level-0="dont_care" pwr_storage-0="dont_care" pwr_storage-1="dont_care" pwr_storage-2="dont_care" storage-0="dont_care" storage-1="dont_care" storage-2="dont_care" storage_index="0" tap_mode="probeonly" trigger_index="0" type="unknown"/>
        </setup_view>
        <trigger_in_editor is_enabled="true" is_node_post_fitting="true" node_name="clk50_div2"/>
        <trigger_out_editor/>
      </presentation>
      <trigger attribute_mem_mode="false" gap_record="true" global_temp="1" name="trigger: 2026/06/01 22:10:31  #1" position="pre" power_up_trigger_mode="false" record_data_gap="true" segment_size="64" storage_mode="off" storage_qualifier_disabled="no" storage_qualifier_port_is_pin="false" storage_qualifier_port_name="auto_stp_external_storage_qualifier" storage_qualifier_port_tap_mode="classic" trigger_in="high" trigger_type="circular">
        <power_up_trigger position="pre" storage_qualifier_disabled="no" trigger_in="high"/>
        <events use_custom_flow_control="no">
          <level enabled="yes" name="condition1" type="basic">
            <power_up enabled="yes">
            </power_up>
            <op_node/>
          </level>
        </events>
        <storage_qualifier_events>
          <transitional>1
            <pwr_up_transitional>1</pwr_up_transitional>
          </transitional>
          <storage_qualifier_level type="basic">
            <power_up>
            </power_up>
            <op_node/>
          </storage_qualifier_level>
          <storage_qualifier_level type="basic">
            <power_up>
            </power_up>
            <op_node/>
          </storage_qualifier_level>
          <storage_qualifier_level type="basic">
            <power_up>
            </power_up>
            <op_node/>
          </storage_qualifier_level>
        </storage_qualifier_events>
        <log>
          <data global_temp="1" name="log: 2026/06/01 22:10:31  #2"/>
          <extradata/>
        </log>
      </trigger>
    </signal_set>
  </instance>
  <global_info>
    <single attribute="active instance" value="0"/>
    <single attribute="config widget visible" value="1"/>
    <single attribute="data log widget visible" value="1"/>
    <single attribute="hierarchy widget height" value="95"/>
    <single attribute="hierarchy widget visible" value="1"/>
    <single attribute="instance widget visible" value="1"/>
    <single attribute="jtag widget visible" value="1"/>
    <multi attribute="frame size" size="2" value="1024,705"/>
    <multi attribute="jtag widget size" size="2" value="334,169"/>
  </global_info>
</session>
